ESP32_RTOS_SDK V1.1.0

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
Event_Info_u Union Reference
WiFi Related APIs » Common APIs

## Data Fields

Event_StaMode_ScanDone_t | scan_done
Event_StaMode_Connected_t | connected
Event_StaMode_Disconnected_t | disconnected
Event_StaMode_AuthMode_Change_t | auth_change
Event_StaMode_Got_IP_t | got_ip
Event_SoftAPMode_StaConnected_t | sta_connected
Event_SoftAPMode_StaDisconnected_t | sta_disconnected
Event_SoftAPMode_ProbeReqRecved_t | ap_probereqrecved

## Field Documentation

Event_SoftAPMode_ProbeReqRecved_t ap_probereqrecved

ESP32 softAP receive probe request packet

Event_StaMode_AuthMode_Change_t auth_change

the auth mode of AP ESP32 station connected to changed

Event_StaMode_Connected_t connected

ESP32 station connected to AP

Event_StaMode_Disconnected_t disconnected

ESP32 station disconnected to AP

Event_StaMode_Got_IP_t got_ip

ESP32 station got IP

Event_StaMode_ScanDone_t scan_done

ESP32 station scan (APs) done

Event_SoftAPMode_StaConnected_t sta_connected

a station connected to ESP32 soft-AP

Event_SoftAPMode_StaDisconnected_t sta_disconnected

a station disconnected to ESP32 soft-AP

The documentation for this union was generated from the following file:

- include/espressif/esp_wifi.h