ESP32_RTOS_SDK V1.1.0

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Public Member Functions | Data Fields
bss_info Struct Reference
WiFi Related APIs » Station APIs

## Public Member Functions

| STAILQ_ENTRY (bss_info) next

## Data Fields

uint8 | bssid [6]
uint8 | ssid [32]
uint8 | ssid_len
uint8 | channel
sint8 | rssi
AUTH_MODE | authmode
uint8 | is_hidden
sint16 | freq_offset
sint16 | freqcal_val
uint8 * | esp_mesh_ie

## Member Function Documentation

STAILQ_ENTRY | ( | bss_info |  | ) |

information of next AP

## Field Documentation

AUTH_MODE authmode

authmode of AP

uint8 bssid[6]

MAC address of AP

uint8 channel

channel of AP

sint16 freq_offset

frequency offset

uint8 is_hidden

SSID of current AP is hidden or not.

sint8 rssi

single strength of AP

uint8 ssid[32]

SSID of AP

uint8 ssid_len

SSID length

The documentation for this struct was generated from the following file:

- include/espressif/esp_sta.h