ESP32_RTOS_SDK V1.1.0

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
softap_config Struct Reference
WiFi Related APIs » SoftAP APIs

## Data Fields

uint8 | ssid [32]
uint8 | password [64]
uint8 | ssid_len
uint8 | channel
AUTH_MODE | authmode
uint8 | ssid_hidden
uint8 | max_connection
uint16 | beacon_interval

## Field Documentation

AUTH_MODE authmode

Auth mode of ESP32 soft-AP. Do not support AUTH_WEP in soft-AP mode

uint16 beacon_interval

Beacon interval, 100 ~ 60000 ms, default 100

uint8 channel

Channel of ESP32 soft-AP

uint8 max_connection

Max number of stations allowed to connect in, default 4, max 4

uint8 password[64]

Password of ESP32 soft-AP

uint8 ssid[32]

SSID of ESP32 soft-AP

uint8 ssid_hidden

Broadcast SSID or not, default 0, broadcast the SSID

uint8 ssid_len

Length of SSID. If softap_config.ssid_len==0, check the SSID until there is a termination character; otherwise, set the SSID length according to softap_config.ssid_len.

The documentation for this struct was generated from the following file:

- include/espressif/esp_softap.h